



 **Specification Sheet**

**PS Part# SC Coil 18/6 LV STOW P**

Construction:

Conductors: 6**-18 AWG (16/30) BC**

Insulation: **Premium Grade PVC** Nom: **0.030” ± 0.004”**

Conductors Color Code: **Purple-Pink-Red-Black-White-Green**

Cable: **5/Conductors Cabled W/Binder Non-Woven Polyester Tape**

Jacket: **Polyvinyl Chloride (PVC) Oil, Moisture, UV Resistant, VW-1**  Nom: **0.065” ± 0.05”**

Jacket Colors: **White , Black (Suffix BK), Clear (Suffix Clear)**

Overall OD: Nom: **0.498” ± 0.05”**

*Note 1: Print/Markings on Product may vary to better suit Industry approvals*

*Note 2: Print Shall be indented. (Not Printed)*

 **(UL) E322633 18/6 STOOW 105C 600V FT-2**

**---c(UL) STOOW 6/C 0.824mm2 (18 AWG) 105C 600V FT-2**

**Wire Processed Under Pendant Systems UL Wire Process # E325558**

Environmental:

**RoHS EU Directive 2011/65/EU (1&2&3), Reach 210,**

**California Prop 65: This product may contain chemicals known to the state of California to cause Cancer.**

**For more information go to www.P65Warnings.ca.gov**

 **NEC Article 400 UL 62 CSA-C22.2-49 OSHA Rating: 105°C 600V**

*“This Cable Design is the intellectual property of Pendant Systems Mfg. intended for use by Pendant Systems Mfg. and their customers. Treat this as a confidential controlled document”*

*Proprietary information*

***THIS DOCUMENT CAN ONLY BE DUPLICATED WITH THE WRITTEN PERMISSION FROM PENDANT SYSTEMS MFG.***